NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

45-35-70/337 Wastes for shower

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[N13](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel) Sanitary appliances and fittings

* [375](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel) SHOWER UNITS
* 377 WET ROOM SHOWERS

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

Product Specification:

KLSD(HM) Linear Shower Drain (HeelMesh)

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: KLSD(SP) Linear Shower Drain (Square Perforated)

• Type: KLSD(HM)80

• Length: 914mm

• Loading class to BS EN 1433: A15

• Fall: No Fall

• Material: 1.4401 (316) stainless steel

• Gully: Central Gully 50mm side outlet (1 ½”BSP)

• Grating: Heelproof Mesh Grating (HM)