NBS Specification:



This product is associated with the following NBS Create clause:

45-25-15/313 Stainless steel bollards

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[Q50 Site/street furniture/equipment](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureBollardsKentIlluminatedBollardKIB1013)

* [190 BOLLARDS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureBollardsKentIlluminatedBollardKIB1013)
* [196 REMOVABLE BOLLARDS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureBollardsKentIlluminatedBollardKIB1013)

Product Specification:

Kent Two Tone Power Bollard – K2TPB-1165

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +353 53 914 3216

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Two Tone Power Bollard – K2TPB-1165

• Type: Buried flange /Cast-in /Fold-down /Removable flip /Removable hidden lock socket /Visible flange

• Finish: Bead blasted /Bright satin finish /Electropolished /Satin 320 grit polish

Suggested Specification:

Kent Two Tone Power Bollard – K2TPB-1165

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +353 53 914 3216

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Two Tone Power Bollard – K2TPB-1165

• Type: Buried flange

• Finish: Bright satin finish